SDV 3.1.7.16 (06.03.2018) Release
- Improve PocketServer Import function: Import new measurement data in existing zone single sub-groups and groups; also over Import->PocketServer-button possible and context menu
- In Gt3S program dialog GSM-/Meas-/Radio-days is substitute with Active days (Out of three check box groups becomes one check box group)
- In Gt3 program dialog GSM-/Radio-days is substitute with Active days (Out of three check box group becomes one check box group). Measurement days in LogN3 related program dialog is not changeable any more.
- Add critical-battery-status-overview table in the end of FTP download for GT3s- and GT3 devices. 
- Bugfix: two devices in map w/ same gps-position cause error
- Expand critical-battery-status-overview table in the end of FTP download for LogN3 device.
- LogN3 Add button to export current measurement data out of the LogN3-measurement-data-table-overview as csv-file.
- Realtimemeasurement for LogP, LogDX and LogD3: improve add-label-function (over context menu)
- Close SDV during Realtimemeasurement cause a confirmation dialog.

SDV 3.1.7.8 (23.10.2017) Release
- LogDX/LogD3 add internal sensor list if sensor files missing
- Map adaption under different screen resolution
- improvement Map View
- Map correlation mode improve 'select two LogN3 devices for correlation'
- add new language: turkish
- add checking for valid device id in new device dialogs
- LogN3 overview click on comment field shows full comment as tooltip
- LogN3 view data dialog: improve index minimum value (show minimum of last period)
- LogN3 improve group read and save data routine
- Gt3S audio sync improvement
- GT3S new dialog: autodetect and autoinsert mode improve close automatically after read one device successfully
- GT3S program dialog: enlarge max characters up to 63 chars (depending on field)
- GT3S group bugfix LogN3 comment (32 chars caused error of program in GT3S programm dialog
- delete subgroup LogN3/LogP bugfix if linked in GT3S group (delete subgroup->delete single devices) 
- new Gt3S Hydorphone
- new Import PocketServer
- Welcome dialog fits to 150% solution
- Daten Logger analyse function improvement
- Tree context menu improve LogN3 context
- Import/Export group bugfix device relation last device

SDV 3.1.7.0 (11.05.2017) release
- GT3S: change color of GT3S symbols from anthracite to ivory-white
- GT3S: improve remote config (add create ftp directory by saving configuration)
- GT3S: improve programming GT3S (PUK-Error)
- GT3S GSM test increase timout of ftp download to 120 seconds
- GT3: unlink devices after successfull programming and link devices after successfull linking
- LogN3: view dialog add "up/down"-arrows to navigate through the measurement days
- LogN3 network mode allow 'read config', 'read audio', 'realtime measurment' via radio interface, read audio block 0, other modes (Lift&shift, patrol) audio block min
- LogN3 read data: data will not be saved if no data available 
- settings-LogN3 add number of values in network mode, use number of values for add new LogN3
- LogP/GT3S new LogP: improve Timeslot 
- LogDX/LogD3 csv export adaption to new LogDX/D3 firmware
- replace google map w/ OSM leaflet

SDV 3.1.6.0 (14.02.2017) 
- add new device GT3S
- add GT3S program dialog
- add GT3S remote config dialog
- add FTP functionality for GT3S
- LogN3/LogP program settings adaption for GT3S group
- new Seba Network tool
- LogD3: improve print of graphic
- Map settings put into menu button 
- remove Reader-2 radio interface option
- improve ftp download logdx after database conversion
- improve logn3 overview table print
- improve total volume in context menu for SebaFlow
- LogD3: program dialog improve variant-channel-relation (2 sensor display)
- graphic: improve printout
 
SDV 3.1.5.0 release (27.06.2016)
- analyses function: improve ftp upload
- improve ftp downlad of gps-coordinates 
- GT-3: remote config add email text and improve synchronisation of the controlls
- GT-3: synchronise firmware version in device setting by measurement data download
- Seba Flow: add volume in total (last week, month, 3 month) in context menu
- LogN3 show data dialog: impr. time calculation (logger time is in measurement period and offset)
- LogN3: limit comment to 32 chars and improve export to commander function
- reduce permitted chars from UTF-7 to Commander3 standard (a-z, A-Z, 0-9, space . - _)

SDV 3.1.4.0 release (25.02.2016)
- analyses function for measurement graphs (addition and substraction of any flow channel of loggers in the same zone)
- save and load logger channel relations of analyses function
- show and hide seperate channels in analyses function
- Curve compare for all data loggers (DX, D3, P-3)
- dynamic load of zones improves start time of the software
- graph: show volumen selected or user defined unit
- graph: display flow channels in two differnt ways - rectangle (former versions only way) and triangle
- realtime measurement: improve statistic (flow counter, pressure, flow)
- P3: add user definded unit
- LogDX/D3: improve event list download via FTP
- LogD3: reset battery counter via context menu
- LogD3: improve Seba Flow functions
- LogD3: show current flow meter counter reading in graph and program dialog
- ftp data download: update battery status
- remove LogD
- devices selectable
- LogP: read measurement data - add radio-fast-mode
- GT-3: improve program dialog 
- GT-3: improve remote config dialog (load config via ftp first, show changes in ftp-config-file)
- GT-3: improve GT-3 config handling (show battery status of LogP)
- GT-3: add function to save default settings of one device in all GT-3 devices in the same group
- GT-3: improve status dialog
- GT-3: improve FTP download
- GSM-Box3: improve program dialog
- ribbon bar improve icon behavior by resizing program window 
- LogN3 improve ftp upload for patrol groups (<ESA threshold level-frequence available)
- Map: improve second screen handling
- LogN3: improve Commander3 export (include GPS coordinates)
- add new Seba GPS mouse 
- SebaNetworkTool: improve imperial-unit-system

SDV 3.1.3.0 release (12.06.2015)
- improve FTP down- and upload
- improve realtime measurement of LogDX/D3
- improve press shock display of LogDX/D3
- LogD3: improve Seba Flow functionality, add battery stage in config downoad via FTP
- map: reducing waiting time to open a map
- GT3: improve remote config file
- LogP: improve remote config file
- improve data reading via radio (RI/RI+ interfaces) for LogP and LogD3
- add slovenish language
- other several imrovements and bugfixes


SDV 3.1.2.0 release(28.08.2014)
- correlation dialog: improve filter, zoom functionality and improve correlation upload
- improve sequence of ftp upload for XML files
- improve XML-zop-file for ftp upload
- map: improve choose of two LogN3 for correlation
- SebaNetWork: show zone point-id and log-id in map
- GT3 config: improve program dialog and LogN3 settings dialog


SDV 3.1.1.0 final release 
- new database
- Integration GT3, LOG D-3
- Correlation with N3 network
- Zone concept to have multiple different devices and N3 groups within one map
- SebaNetworkTool to draw pipenetworks with pipe data, distances, etc. which can be used for correlation
- zone/pipenetwork upload to SebaCloud
- display/hide single channels of dataloggers
- Integration SebaFlow

Please note:
SDV 3.1.x is an upgrade for SDV 3.0.x. The upgrade is irreversible. The database will be transfered to the new one during the first start of the new SDV 3.1.1.0. It is not possible to import/export zones between the different versions of SDV 3.0.x and SDV 3.1.x. Please import all zones you need into SDV 3.0.x before you upgrade to SDV 3.1.x.

SDV 3.0.6.1 (05.07.2013)
- LogP: Cursor function avaliable
- LogDX: New error text for curve analyse function
- LogDX: read press shock file from reader3 considering DST 

SDV - 3.0.6.0 (14.06.2013)
- official release

SDV - 3.0.5.4
- Commander3 data import: improve import of audio data
- LogDX show graph: improve analyse function

SDV - 3.0.5.2
- CSV-Datei Export: new settings availiable
- LogDX show data: improve volume counter

SDV - 3.0.5.0 (08.04.2013)
- official release
- LogP configuratiton: add daylight flag
- GSMBox3 ftp-download over http-based proxy server possible
- LogDX take care of the daylight saving time, it the Logger was programed in winter time
- LogDX Config direct upload to Server without local program

SDV - 3.0.4.6 (28.03.2013)
- ftp-settings tab: split "use own server" into "use own FTP server" and "use own email server"
- LogN3 edit dialog: show saved gps-coordinates, fix of a special problem on a few computers 
- Map: improve show data with double click after scrolling 
- fix some wrong translations in polish, spanish, czech, dansk and frensh (1% instead %1 -> memory error, % 1 instead of %1)

SDV - 3.0.4.5 (22.03.2013)
- add LogRI Plus (LogRI +) Firmwareupdate and comunicaton device list at info-window
- LogDX/LogP program dialog: improve handling of time settings (if <1970)
- LogP Autoscale to remove the ground noise effect
- LogDX/LogP sdb file import direct open the Readerbox Root 
- LogP Print Measurment Record avalialble
- LogN custom & seba-logo print
- improve import/export zone
- LogDX realtime measurement digital dialog: improve handling of sign slave channels
- LogDX channel config dialog: improve sign slave input type channel selection
- LogN3 show data dialog: improve comment edit (automatic word wrap)
- LogN3 New Dialog: add automatic comment check box
- LogN3 show measurement data dialog: stop audio if next/previous LogN3 is choosen
- LogN3 view config dialog: improve error message handling
- LogDX Eventlist show detail

SDV - 3.0.4.4 (13.03.2013)
- LogP: sdb & press shock files import

SDV - 3.0.4.3 (12.03.2013)
- SDV Tree: remove Items using delete key
- special version for Windows XP

SDV - 3.0.4.2 (06.03.2013)
- LogP/LogDX config channel improve press shock threshold (0.0 not allowed anymore)
- LogDX TDM 200 program dialog: set channel 3 (signslave for channel 2) to backward mode before the programming of the device
- LogDX realtime time measurement graph: fixing problem in forward-mode of a signslave channel
- add language simplified chinese (100%)
- LogDX real time measurement digital: improve handling of signslave channels (hide)

SDV - 3.0.4.1 (01.03.2013)
- GsmBox3 config dialog: change default values for email and sms uploads (in case of alarm)
- LogDX: Print with Company Logo
- LogDX: Curve analyse Substration & Addition with histroy info
- LogDX: sdb & press shock files import 
- (LogN3: recieve GPS position from a GPS device)
- LandMap & LogN3 Listview: improvment & bugfix 
- LogN3: add import of Reader3 data (measurement data and pressure shocks)
- LogN3 overview spreadsheet improve sort function (print)
- LogDX channel config dialog: pressure-sensors - add custom unit text (max. 5 characters) and related min./max. real values

SDV3 - 3.0.4.0 (21.12.2012)
- official release

SDV3 - 3.0.3.22 (XX.12.2012)
- LogN3 read config dialog: improve - read also if LogN3 in config mode
- improve FW update for LogDX
- Tree: map always at the first position in a zone
- LandMap : Find LogN3 in the corresponding place in LandMap and other important improvements
- LandMap : new Loggers in the zoom window
- LogDX : User-defined Unit displayed correctly
- Templetes internetprovider improve STC Saudi Arabia
- LogDX: Config file complete upload
- LogDX: Config from ftp-server download

SDV3 - 3.0.3.21 (10.12.2012)
- Landmap: new zoom function(eagle eye overview) and improvement of print function
- LogD/DX show measurement data list dialog: improve language realations of the dialog buttons
- hide LogDX edit dialog and remove comment edit in LogDX new dialog: comment only over program dialog possible
- LogDX read data: hide check box "read press shock", if press shock is not possible or not activated
- LogDX GSM test dialog: imporve language text (SMS)

SDV3 - 3.0.3.20 (04.12.2012)
- Import zone: improve export and import of LogD measurment data

SDV3 - 3.0.3.19 (04.12.2012)
- LogN3 show data: add comment-edit

SDV3 - 3.0.3.18 (26.11.2012)
- export a zone for an other SDV (sqlight-database-format)
- import a zone from an other SDV (export) (sqlight-database-format)
- tree sort by name, always in a level
- LandMap: Gps position of Loggers correct located
- LandMap: parameters saved after the porgram is closed
- GSMBox3: Remote Config Audio Request improvement
- LogDX: show the Measdata in within the determined time space
- Tree: add waitcursor during delete elements function
- sqlight user_version = 1 (for export/import)

SDV3 - 3.0.3.17 (14.11.2012)
- LogDX channel settings config dialog: improve relation between qm/h and l/h (autorecalculation when type of sensor will be changed)
- LogDX: Ftp-download group download avaliable

SDV3 - 3.0.3.16 (12.11.2012)
- GSMBox: Ftp-download of audio files avaliable for both bin_ and wav-file
- GSMBox: improve Ftp-download
- LogDX channel settings conifg dialog: improve user defined input settings (position after decimal point)

SDV3 - 3.0.3.15 (08.11.2012)
- improve FW update
- LogDX: improve Ftp-download (attach the files of the same measurement together after error occurs on ftp files

SDV3 - 3.0.3.14 (07.11.2012)
- firmware update: add automatic detection for LogDX, LogN3, LogP and Log Rep
- LogDX TDM 200 channel config dialog: improve use of sign channel settings
- LogP config dialog: add record time span check and automatic correction
- LogDX: CSV-export the decimal separator compatible with system settings
- LogDX new dialog: add id detection and auto insert
- LogN3 show config dialog: improve measurement time span 
- LogDX config dialog: improve relations between sample time and channel alarm thresholds with pulse as input type
- LogDX cursor function avaliable in Graphic
- Tree: improve zone info (number existing devices in a zone - empty zone shows 0 insteat of 1)

SDV3 - 3.0.3.13 (26.10.2012)
- LogRI improve FW update handling (animated scrollbar)
- LogDX variant TDM: disable channel 3 (hard direction of flow - no change of flow direction via SDV possible)
- LogDX read measurement data: improve reading time
- LogD program channel dialog: improve user defined handling of unit field after pulse was selected (enabled now)
- LogD program dialog: synchronice comment in dialog with comment in tree
- FW udpate: no RI/Reader 3 connected - only one error message "communicaton device missing"
- LogDX program dialog: set local time zone if FW-version of the device is equal or higher 1.01.18
- LogDX: print detail channel information
- LogDX: improve Ftp-download
- LogN3: improve print of LogN3 group talbe overview (more than 40 are possible now)
- Gsmbox3: new link for the Webtool

SDV3 - 3.0.3.12 (22.10.2012)
- LogP: add measurement report dialog (print still missing)
- LogDX: add 12 more variants for loggeres with 2 pressure channels
- LogDX show event list dialog: improve usb reading of event data
- LogD config dialog: improve info field current time after programming (time shift correction)
- LogDX: print detail channel information
- LogDX: improve Ftp-download

SDV3 - 3.0.3.11 (16.10.2012)
- LogDX: add dialog for measurement report for every measurement data set (no limit of report length)
- LogP: add dialog for measurement report for every measurement data set (no limit of report length)
- LogDX/LogD program channel dialog: add "type of sensor" field
- LogDX: Determine the length of measdata paket in Ftp file by pattern delimiter.
- LogDX: possible Measdata Report print after Graphic printed.
- LogP new dialog: error message if device ID is zero (no ID entered)
- LogP program dialog: message if measurement period is less than 10 times of the measurement intervall
- LogP new dialog: insert new device if auto insert check box is activated an a device is detected (auto detection activated)
- LogDX: MeasdataReport add report dialog (improvement)
- LogP: by realtime measurement won't save data after stop.
- LogP: Label immediately editable after new insert.
- LogP: Textfield adaptive to the text length.
- LogDX: download separate Ftp-measdaten of one measurment in one dataset.
- LogD: use corrfactors in the measdata-calculation.
- LogD gsm config dialog: demo mode for ftp server changed. Updatet to new valid account data. 

SDV3 - 3.0.3.10
- internal use R&D

SDV3 - 3.0.3.9 (24.09.2012)
- LogD: new calculation function for the Graphic
- LogP: autoscale at the begining of Graphic loading
- LogP: print function is through print menu available
- improvement of languages portuguese and spanish

SDV3 - 3.0.3.8 (21.09.2012)
- LogN3 add read and show config dialog
- LogDX ftp config header packet number upload.
- LogDX always try to create ftp directroy when the ftp active is.
- LogDX ftp config file name in lower case.
- LogDX new ftp steptest event from ftp download
- LogDX timestamp in ftp file name in modifytime in DB save.
- LogP By realtime measurement always send short preample even still in listen-modus.
- LogD channel settings dialog: improve alarm levels (min/max)

SDV3 - 3.0.3.7 (14.09.2012)
- changes in seba demo database: logP with new settings and new measurement data
- improve of import from Commander 3
- LogDX add remote configuration via FTP server
- LogDX improve current loop measurement

SDV3 - 3.0.3.6 (12.09.2012)
- LogDX demo-server location changed - first step for common ftp-account for all devices
- LogDX config channel dialog: add 'check FTP for settings' in alarm settings
- tree: add TDM 200 icon
- GSMBox3: romate configeration upload & ftp-directroy auto create
- LogDX GSM test dialog: add button to read the event list (check for the result of the gsm test)
- LogDX channel alarm settings dialog: check FTP for new config - activate SMS alarm automaticaly, message if SMS settings missing

SDV3 - 3.0.3.5	(30.08.2012)
- LogP add Group programming dialog
- LogP add new Button for CSV-export of selected dataset in Data-List
- LogP Stop Send Command after digital Realtime Measurement is stopped
- LogP Ribbon Button in Context Catagory fits the langer Text for all Languages
- LogD change P2 variants from channel 1/3 to 1/2
- LogDX Graphic show min-value correctly 
- LogDX Ftp Pressshock files download
- LogP  Realtime Measurement dialog breakout after error reading the first Measvalue
- add language portuguese
- LogP/LogN3 new dialog - disable field LogID if auto detect is selected

SDV3 - 3.0.3.4
- internal use R&D

SDV3 - 3.0.3.3 (03.08.2012)
- LogN3 read measdata via radio - handling of an offset: save measurement data in Commander3/Reader3 conform format
- LogN3 ESA value correctly calculated with Measdaten with Offset.
- LogN3 show the Graphic window text with Document title.
- add russian as new language
- LogP expand functionality - new FW for LogP needed!
- LogP new-LogP-dialog: improve autodedect
- LogDX show 35 bar instead of 40 bar if a 40 bar sensor is in use (also matter units psi and MPa)
- LogP improve handling of convertion factor
- LogDX FTP remote Config, create new directory on FTP server for the first device-program
- LogDX hide Channel 3&4 und TDM mode.
- LogN3 add new animation and feedback messages for FTP download
- LogP program dialog - add estimated record time
- LogDX add special handling of the channel settings for TDM 200, change dialog titles from LogDX to TDM 200, for the TDM variant of the LogDX
- SDV Aboutbox add a list of all the Communication Devices and the firmware version that are active connected to the PC 
- LogP  correct the number of measdata when read local measdata from the device
- Graphic and Show Data List sample interval are displayed in days-hours-minutes-seconds form instead of seconds only.
- Graphic deactivate panning with keyboard in overview graphic, instead that the zoom box moves with the keyboard input
- LogP improve read data dialog (press shocks will be read also if no new data is available).
- LogP graphic open afte read local measdata without pressshock.
- LogP show Pressshock outof the range of measdata
- LogP Realtime measurement digital only on Channel showed in dialog

SDV3 - 3.0.3.2
- internal use R&D

SDV3 - 3.0.3.1(19.06.2012)
- LogN3 Ftp Internet Connection(PASV) improved, Gps-coordinates of the Zone download from Ftp-server.
- LogP  Realtime measurement in digital form. CSV file export. Markers of Pressshock in Graphic are fixed.
- LogD LogDX  Ftp Internet Connection(PASV) CSV file export(group-auto) improved.

SDV 3 - 3.0.3.0 (06.06.2012)
- LogN3 import from Reader 3 integration in import dialog, add import symbol in LogN3 ribbon bar part
- LogP program dialog: yes/no-message box to make sure, that the user knows, that data on a LogP will be lost, if he programming it. 
- LogD improve csv-export under windows xp
- LogDX add graph arithmetic (addition) in a new graph dialog
- costumer settings: user FTP settings used in ftp-download as common settings

SDV 3 - 3.0.2.2 (31.05.2012)
- LogD program dialog sensors: add psi and MPa for pressure sensors

SDV 3 - 3.0.2.1 (29.05.2012)
- LogDX program dialog: differ between LogDX and TDM 200 variant in dialog name
- LogDX program dialog: show externally supplied devices in battery status field.
- LogDX show data: differ between LogDX and TDM variant.
- LogDX read data: no automatic show of data, if no data is available (now only one message window "no data available")

SDV 3 - 3.0.2.0 release (24.05.2012)
- GSMBox3 program dialog: ftp-path always "gsmbox3/"
- LogD add import of groups via FTP

SDV 3 - 3.0.1.24 (23.05.2012)
- LogN3 view data dialog: improve calculation of the leak value with offset in measurement data.
- LogDX program dialog: add psi and MPa as unit types for ratiomatric sensors

SDV 3 - 3.0.1.23 (16.05.2012)
- LogDX program dialog for channels: immprove handling "per second"/"per hour", all unites by custom unit now allowed
- LogDX Read Event List via USB 
- LogN3 New instance: change standard value for time slot (to 0xff).

SDV 3 - 3.0.1.22 (10.05.2012)
- LogDX improve realtimemeasurement digital
- LogDX add edit dialog
- LogDX print data: improvement - add comment text in print (first half graph, second half comment)
- LogDX config channel dialog: improve refresh of dialog text after changing puls-second/hour setting

SDV 3 - 3.0.1.21 (08.05.2012)
- LogDX program dialog: TDM variant - hide alarm inputs and alarm via relays
- LogDX program dialog: add unser defined unit text
- LogDX daylight saving time: add interpretation to handle the local time of a LogDX depending on daylight saving time
- Templetes Internetprovider: add Orange (Poland)
- LogDX add dialog for GSM test
- LogDX improve realtimemeasurement

SDV 3 - 3.0.1.20 (03.05.2012)
- testversion for development - multible versions with this number possible. Only for development!!!

SDV 3 - 3.0.1.19 (02.05.2012)
- LogDX program dialog: hide alarm settings if LogDX is a TDM (product ID: 12345)
- LogDX program gsm dialog: restructor of the functional blocks (sms, email, ftp), show/hide blocks depending on activating of functionality.
- GSMBox3 add FW update
- LogDX show data improvements (e.g. add current channel, add signed slave channel)

SDV 3 - 3.0.1.18 (24.04.2012)
- LogDX program dialog: add daylight saving time, but still no interpretation in the handling the local time of a LogDX 
- common settings: improve FTP settings - use own server button.

SDV 3 - 3.0.1.17 (24.04.2012)
- LogDX config channel dialog: improve handling (hide/show alarm boxes), automatic activation of alarm if alarm-channel is selected
- LogDX settings: change of the channel-settings - no work with former LogDX settings possible any more!!!!
- LogDX programm settings dialog: read/write settings: change in radio-protocoll. avoid communication with older LogDX!!

SDV 3 - 3.0.1.16 (23.04.2012)
- LogDX config dialog: improve handling of channel handling
- LogDX program dialog: improve adoption of status register in function of read settings
- LogDX read measurement data: improve add new data

SDV 3 - 3.0.1.15 (17.04.2012)
- LogDX add realtime measurement
- LogDX improve read data press shock
- improve handling of current measurement

SDV 3 - 3.0.1.14 (17.04.2012)
- Templates internet provider add new: Plus (Poland)
- LogDX config channel dialog: improve selection of sensor type if channel 3 is available
- LogDX config dialog: add battery status

SDV 3 - 3.0.1.13 (13.04.2012)
- LogDX improve storage of the settings after a successfull programming of the device.
- LogDX program dialog: message after successfull programming.

SDV 3 - 3.0.1.12 (12.04.2012)
- LogDX realtimemeasurement
- LogDX program dialog: GSM test
- LogDX program dialog: improve handling of alarm settings

SDV 3 - 3.0.1.11 (29.03.2012)
- Reader 3 data import: improve import of measurement data not in leak mode. Also calculate ESA value.

SDV 3 - 3.0.1.10 (28.03.2012)
- testversion for development - multible versions with this number possible. Only for development!!!

SDV 3 - 3.0.1.9 (28.03.2012)
- LogN3 show data: improve display of the frequency value, if the logger is not in leak mode (zone in patrol group mode)
- Reader 3 data import: improve import of measurement data not in leak mode.

SDV 3 - 3.0.1.8 (21.03.2012)
- testversion for development - multible versions with this number possible. Only for development!!!

SDV 3 - 3.0.1.7 (26.03.2012)
- LogDX add indiviual symbol for LogDX (LogD green colored)
- improve de- and endcryption of passwords

SDV 3 - 3.0.1.6 (21.03.2012)
- testversion for development - multible versions with this number possible. Only for development!!!

SDV 3 - 3.0.1.5 (20.03.2012)
- LogDX Graphic for measurement data
- LogDX Ftp Download for single device
- LogDX CSV file export manual and automatic
- LogDX Show historical Measurement list dialog
- LogDX program dialog: include customer FTP/Email settings
- LogD program dialog: include customer FTP/Email settings
- common Settings: add FTP/Email settings
- GSMBox3 program dialog: include customer FTP/Email settings
- LogN3 read data:improve handling of LogN3 in config mode
- New installation of the SebaDataView: New demo folder for LogN3 and LogP

SDV 3 - 3.0.1.4 (05.03.2012)
- improve error message handling by RF crc errors
- Land map dialog: improve import of google map snap shots

SDV 3 - 3.0.1.3 (01.03.2012)
SDV 3 - 3.0.1.2 (29.02.2012)
- pipe network dialog (landmap): improve google maps import with slow internet connection
- LogN3 table overview: improve table reloading
- LogD Import FTP data: Bugfix

SDV 3 - 3.0.1.1 (27.02.2012)
- testversion for development - multible versions with this number possible. Only for development!!!

SDV 3 - 3.0.1.0	(24.02.2012) - frist official release
- LogD show data dialog: bugfix for calculation of voltage, ampere and frequency
- Windows arrangement in different ribbon tabs intigrated

SDV 3 - 3.0.0.44 (22.02.2012)
- About dialog: improve related pdf documents 
- LogN3 table overview: add note-symbol if audio data is available

SDV 3 - 3.0.0.43 (22.02.2012)
- LogN3 data import from Reader3 with automatic source detection
- LogN3 table overview: add sorting by device id and comment
- LogN3 table overview: improve store and restore last sort-settings
- LogN3 show measurement data dialog: play audio sound continuesly in a loop
- LogD/LogDX change text in GSM configure dialog in category "internet settings" (server address (APN))
- Templetes Internetprovider: add Web2 (Saudi Arabia)
- Tree: add sort functiality by sorting by ID and sorting by comment ascent and descent
- Import LogN3 data from Commander3: improve by adding GSM Box3 import
- About dialog: add button to show the help file (pdf document)
- Settings dialog: add button to open the explorer with the path to the database file of the SDV

SDV 3 - 3.0.0.42 (17.02.2012)
- LogN3 table overview: improve waiting time for building the overview.
- LogN3 data view: print dialog - add LogN3 details
- LogN3 data view: print preview is available
- LogN3 data view: resize dialog window
- Import LogN3 data from Commander3 changed to: add only new data or rebuilt under a new zone name.
- Windows alignment for data windows
- Land map dialog: add delete function
- Land map dialog: hide LogN3 devices when not in leak modus or when no data available
- Land map dialog: add color modes for frequency, level and ESA
- Land map dialog: save and restore the choosen critera

SDV 3 - 3.0.0.41 (17.02.2012)
- testversion for development - multible versions with this number possible. Only for development!!! (including also changes of 3.0.0.42)

SDV 3 - 3.0.0.40 (09.02.2012)
- LogN3 Realtimemeasurement: Leakvalue - change of level unit from "%" in "dB"
- LogN3 table overview: improve table reloading
- LogN3 table overview: store and restore last sort-settings and the mode (ESA/frequence/level)
- LogN3 show measurement data dialog: add LogN3-ID and comment in title of the dialog
- Tree: store (exit SDV) and restore (start SDV) last acitve zone in Tree 
- LogP show graph dialog: general improve
- LogP show graph dialog: add labels for pressure shock, same functionality for LogP and LogDX 
- LogP show graph dialog: add makers for pressure shock
- UTF7 handling: improve handling - after handling of a wrong character input the cursor is set to the correct position in the edit control
- LogD config channel dialog: improve selected of sensor types - permanent installed presure sensors - no choice possible anymore
- LogD volume unit always in m3
- LogD csv data export in m3 and considering watermeter start value
- Land map dialog: add maximize/minimize symbols
- Tree: Copy LogN3 devicegroup or a single LogN3 device - dialog group mode will appear when no LogN3 group mode in the destination group is slelected

SDV 3 - 3.0.0.39 (30.01.2012)
- testversion for development - multible versions with this number possible. Only for development!!!

SDV 3 - 3.0.0.38 (24.01.2012)
- LogD config channel dialog - improve storage andd display of the sensor settings
- LogD automatic CSV-export function also available for FTP download 
- LogP show measurement data - add graph overview window

SDV 3 - 3.0.0.37 (18.01.2012)
- status text in red color
- Tree: context menu - import/export
- new language: romanian
- new language: japanese

SDV 3 - 3.0.0.36 (12.01.2012)
- FTP-Import GSM-Box3: Handling of import of audio-files - no message box, when no audio file is available on the ftp-server and automatic finisching of the import dialog box.
- ViewTree: amount of devices in paraetheses shown in the name of a zone and in the devicegroups (e.g. Baunach (17), LogN3 (14))
- ViewTree: LogN3 groupmode shown in the beginning two characters in the name of a zone (e.g. L_Baunach ... L_ stands for lift&shift mode, P_ stands for patrol mode, N_ stands for network mode)
- New LogN3: improve interaction between auto-detect and auto-commentar
- New LogN3: message, if device already exists
- ViewTree: context menu - copy zone/device group - message how to copy a zone/device group/device with drag-and-drop

SDV 3 - 3.0.0.35 (09.01.2012)
- Tree: sorting in alphabetic order
- LogN3: show measurement data - after double click latest data will be shown
- New Devices in a zone also LogD and LogP possible in network-mode
- FTP-Import GSM-Box3: Handling of wrong measurement files version 1 (avoid logID = 0)

SDV 3 - 3.0.0.34 (21.12.2011)
- SDV can only started one time
- Zone: new-zone-dialog: commentary character check (only UTF7 allowed because of the Commander 3) - erease not allowed characters automatically.
- LogN3 table overview: switch between frequency, level and ESA value
- LogN3 table overview: maximize and minimize possible
- LogN3 table overview: sorting by frequency, level and ESA value
- LogN3 table overview: time filter - limit shown measurement date in the table for a period of 30 days
- Web Tool: connection to LogN3/GSMBox3 Seba Server, displayed in a window in the SDV

SDV 3 - 3.0.0.33 (13.12.2011)
- LogN3: Datenimport Commander: Verbesserung

SDV 3 - 3.0.0.32 (09.12.2011)
- LogD: Nach Neuanlage eines LogD ist das Konfigurieren jetzt auch über die Eingabe der Variante (PN) (Variant-Button) des LogD möglich. Die Einstellungen können abgespeichert werden, auch wenn der nicht erfolgreich programmiert ist (Save-Button)
- LogD: Verbesserung Startzeitpunkt Datenaufzeichnung

SDV 3 - 3.0.0.31 (02.12.2011)
- Neue Icons in Ribbonbar
- LogN3 Ausdruck der Messdaten der ausgewählten Messdatengrafik, Druckvorschau

SDV 3 - 3.0.0.30 (30.11.2011)
- LogD: Verbesserung FTP-Import

SDV 3 - 3.0.0.29 (29.11.2011)
- Einstellungen: Zuordnung der Sprachen
- LogD: Verbesserung Contextmenü

SDV 3 - 3.0.0.28 (28.11.2011)
- LogD: Echtzeitmessung als Dialog
- LogD: GSM-Einstellungen: Verbesserung Auswahl FTP-Demoserver und Email-Demo-Einstellungen
- LogD: Verbesserung Dialog Konfigurieren Kanal/Sensor: Anzeige, wenn im LogD kein Sensortyp steht.
- LogD: m3/h und l/s im Programmierdialog umschaltbar und wird entsprechend in der Grafikdarstellung angezeigt 
- LogN3: Übersichtstabelle ausdrucken
- LogN3: Druckvorschau Übersichtstabelle drucken
- neue Sprache: dänisch
- neue Sprache: polnisch

SDV 3 - 3.0.0.27 (11.11.2011)
- LogD: Bei manuellem Export der CSV-Datei kann der Speicherort und der Dateiname individuell gewählt werden.
- LogD: Programmieren: Umstellung/Verbesserung der LogD-Zeit auf GSM in allen Zeitwertvorgaben
- Überarbeitung des Sprachfiles: Umstellung Begriff "Gruppe" auf "Zone" in Nachrichtentexten
- LogN3 neu anlegen: Verbesserung Zusammenspiel der Checkboxen und Buttons.

SDV 3 - 3.0.0.26 (07.11.2011)
- GSM-Box3 Programmierdialog: "Export" Schaltfläche ausgeblendet.
- Baumansicht: "root"-Ordner wurde in "SebaData" geändert.
- Umstellung des Begriffs "Gruppe" auf den Begriff "Zone", die Untergruppe wird zur Gerätegruppe
- Anpassung Texte in den Dialogen "LogN3-Gruppenmodus wählen" und "GSM-Box3 programmieren"
- LogD Programmieren: Verbesserung der Kommunikation PC-Reader3-LogD
- LogD Programmieren: Kanal-Durchflussmessung: Zählerstand programmierbar
- LogD Programmieren: Kanal Darstellung l/sec und m3/h auswählbar für XGraph-Datenanzeige (in Vorbereitung)
- LogD FTP-Import Messdaten
- LogD FTP-Import Event-Liste
- LogD Automatischer Datei-Export im CSV-Format bei auslesen der Messdaten über Funk/USB
- XGraph Verbesserung Anzeige Max/Min Alarm

SDV 3 - 3.0.0.25 (26.10.2011)
- Testversion(en) für die Entwicklung 

SDV 3 - 3.0.0.24 (26.10.2011)
- LogP: Verbesserung Daten auslesen (Überarbeitet für SDV und LogP)
- GSM-Box3 Neuanlage: Verbesserung: Wird die Neuanlage einer GSM-Box abgebrochen, ist nicht mehr automatisch die Gruppe im Netzwerkmodus
- LogD: Integration GSM-Test-Funktionen (nach Vorbild SDV2)
- LogD: Importieren (download) der FTP-Daten vom FTP-Server in die SDV
- LogN3: FTP-Import: Verbesserung download Audiodateien
- Gruppe editieren Verbesserung 

SDV 3 - 3.0.0.23(17.10.2011)
- GSM-Box Programmieren: Default-Einstellungen bei neuangelegter GSM-Box integriert.
- Kartenanzeige: Geräte mit 0-Koordinaten werden nicht mehr mit angezeigt.
- Kartenanzeige: Ausschnitt bei vorhandenen GPS-Koordinaten verbessert.
- Google-Map-Modus wird nach der Benutzerauswahl gespeichert (Markierungen werden nicht mehr übernommen)
- LogN3: FTP-Import Audio-Dateien (Netzwerkgruppen)
- LogD: Anzeige Messdaten Vebesserung/Erweiturung durch Funktion Messung
- LogD: Anzeige Messdaten Funktion Cursor (Detailanzeige Messdaten an der Kurve) entfernt. Grund: weiterer Entwicklungsbedarf

SDV 3 - 3.0.0.22 (30.09.2011)
- Auswahl Gruppenmodus: korrekte Gruppe wird übernommen (Korrektur zu 3.0.0.21)
- LogN3: Bei der Initialisierung wird das Statusbyte mit 3 (Batteriestatus OK) initialisiert.
- LogD: Dialog Programmieren GSM-Einstellungen SMS/Email-Summary täglich/wöchentlich-Abhängigkeit verbessert.
- Templetes Internetanbieter Ergänzt mit Q-Tel (Katar)
- Templetes Internetanbieter Ergänzt mit Orange (Israel)
- LogD: Anzeige Messdaten Verbesserungen (min./max.-Alarm, Durflusszähler)

SDV 3 - 3.0.0.21 (16.09.2011)
- LogN3 Gerät neu anlegen: Verbesserung Darstellung Texte, Autokommentar jetzt gleich wie bei Commander 3 (z.B. LOG 001 statt LogN3-01) 
- Verbesserung in der Zusammenspiel der verschiedenen Gruppenmodi zu den Geräten. Z.B. kann in einer Netzwerkgruppe nur eine GSM-Box3 und mehrere LogN3 angelegt werden. Aber kein LogD. In eine Lift&Shift-Gruppe kann keine GSM-Box angelegt werden.
- Grafische Darstellung LogD Erweiterungen (Messen, Verschiebung, Alarmschwellwert Darstellung als Linien für min/max), Ansichtsbereich einstellbar (Stunde/Tag/Woche/Monat)

SDV 3 - 3.0.0.20 (09.09.2011)
- Testversion(en) für die Entwicklung (Manuel)

SDV 3 - 3.0.0.19 (07.09.2011)
- Korrektur Listen sensor_logd.ssf und sensor_logdx.ssf (Frequence counter, i2S), Aktualierung bei Installation ab dieser Version
- LogD Kanäle: Verbesserung Auswahl der Sensoren - unstimmiger Werte konnten zu einem undefinierten Zustand des Sensors führen
- LogD Export aktuelle Messdaten als CSV-Datei mit Spalte Gesamtvolumen bei Durchflussmessung
- LogD Verbesserung Ansicht Messdaten Zoomfunktion

SDV 3 - 3.0.0.18 (06.09.2011)
- Neuanlage Geräte und LogN3 editieren: Kommentar nur noch im Format UTF-7 möglich
- LogN3 Datenanzeige: Auswahlfeld für  historische Daten jetzt nach dem Datum absteigend sortiert.
- LogN3 Datenanzeige: ESA/Level/Frequenz wird korrekt angezeigt
- Datum- und Zeitformat vereinheitlicht auf Jahr-Monat-Tag und Stunden:Minuten:Sekunden (z.B. 2011-08-31, 13:52:03)
- LogD Anzeige: Labels eingefügt
- LogN3 Datailanzeige Tabelle Gruppe: Anzeige der Werte inkl. Farbe verbessert.
- Gruppenmodus wird nicht mehr bei der Neuanlage einer Gruppe ausgewählt, sondern erst, wenn in einer Gruppe der erste LogN3 neu angelegt wird.
- neue Sprache: tschechisch

SDV 3 - 3.0.0.17 (23.08.2011)
- Anwendungssettings: Erweitert um default-Einstellungen für den LogN3 in allen drei Gruppemmodi (Patrouillier-, Lift&Shift- und Netzwerkmodus)
- Verknüpfung der default-Einstellungen für den LogN3 mit dem Einzel- und Gruppenprogrammieren.
- Netzwerkmodus: Einlesen von GSM-Box3 bereitgestellten Daten vom FTP-Server (LogN3-Geräte).
- Gruppen im Netzwerkmodus: Auskommentieren bzw. mit Hinweistext nicht ausführen von Funktionen für das LogN3-Gerät (Daten auslesen, programmieren).
- Gruppenimport Commander 3: Hinweistext zum Gruppenimport erweitert, Abfangen Import einer historischen Gruppe mit Hinweistext (führte zu fehlenden Daten)
- Gruppenimport Commander 3: Verbesserung Import historischer Daten vor dem 26.07.2011. Sie konnten vorher nicht importiert werden. 

SDV 3 - 3.0.0.16 (29.07.2011)
- Sonderversion Produktmanagement (nur LogN3/GSM-Box 3)

SDV 3 - 3.0.0.15 (28.07.2011)
- LogP: Verbesserung Einlesen Messdaten, Verbesserung Einlesen Druckstoss

SDV 3 - 3.0.0.14 (19.07.2011)
- Sprache Spanisch funktioniert und kann jetzt ausgewählt werden.
- LogD: Ausdruck vom Messgraph - Neu
- LogD Messgraph Verbesserung Auswahl Kontextmenü, Abfangen Fehler bei Funktion Messen

SDV 3 - 3.0.0.13 (15.07.2011)
- Rohrnetzplan: Verbesserung: Durch Doppelklick auf das Kartensymbol im Baum lässt sich wieder die Karte öffnen.

SDV 3 - 3.0.0.12 (14.07.2011)
- LogN3 Gruppen-Programmieren: Sind am Ende der ToDo-Liste Geräte noch nicht programmiert, wird wieder ab dem ersten Geräte in der Liste weitergemacht.
- LogN3 Gruppe-Auslesen: Lift&Shift-Modus: Bei einem Auslesefehler wird ein Gerät jetzt mehrfach ausgelesen. Erst nach mehreren Versuchen wird das nächste Gerät in der Liste genommen.
- LogD Messdatenanzeige: Übersichtsfenster im oberen Drittel und Detailanzeige im unteren Bereich, Zommausschnitt in der Übersicht
- LogD Messdatenanzeige: Detailanzeige der Kanäle (Min, Max, Summe)
- LogD Programmieren: Verbeserung Sensoren, Ergänzung einer Variante
- MenuExport: Gruppenexport für den Comander 3 
- LogN3 neues Gerät anlegen: Bei der manuellen Eingabe wird nach den einfügen das Eingabefeld für die LogN3-ID gelöscht und der Fokus darauf gesetzt.
- Gruppe: Es kann jetzt nur noch eine GSM-Box 3 in einer Netzwerkgruppe angelegt werden. D.h. Es ist nicht möglich, eine GSM-Box 3 anzulegen in einer Lift&Shift oder Patroliergruppe, sowie, wenn bereits eine GSM-Box 3 in der Netzwerkgruppe vorhanden ist.
- GSM-Box3 Programmieren: Button zur Übernahme der Einstellungen in die Datenbank (ohne Export) eingefügt.
- LogP Messdaten auslesen: Since last read eingeführt, Verbesserung des Ablaufs, wenn beim auslesen Übertragungsfehler auftreten (die Daten bis zum Abbruch werden gesichert)

SDV 3 - 3.0.0.11 (21.06.2011)
- Testversion(en) für Entwicklung (Tristan)

SDV 3 - 3.0.0.10 (15.06.2011)
- Sonderversion für Produktmanagement

SDV 3 - 3.0.0.9 (15.06.2011)
- Import LogN3-Daten: Routine zur Behandlung der älteren Commander 3 - Dateien. Ältere Messdaten können so noch vom Commander 3 importiert werden. Stichtag ist der 01.07.2011! Wird nicht rechzeitig ein Firmwareupdate im Commander 3 gemacht, können die Messdaten, die nach den Stichtag eingelesen wurden, nicht mehr in die SDV importiert werden.
- Import LogN3-Daten: Verbesserung Importroutinen bei historischen Daten. Zurückgesetzte Daten vom Commander 3 werden nicht mehr importiert.
- LogN3 Übersicht Messdaten: 1. Spalte (LogN3-ID und Kommentar) und 1. Zeile (Datum) sind beim scrollen fixiert.
- Rohrnetzplan: Verbesserung in der Zoomfunktion (Scrollen)
- Rohrnetzplan: Import Google-Maps Karten jetzt mit GPS-Koordinaten zwischen -180 Grad und +180 Grad möglich.
- Ungarisch als 5. Sprache aufgenommen.

SDV 3 - 3.0.0.8 (07.05.2011)
- Firmwareupdate: Fehlende Texte ergänzt. Verbesserung beim Abbruch während eines Updates.
- Firmwareupdate: LogP zugefügt, Endungen auf Wunschendungen anderer Entwickler angepasst.
- LogN3View: Daten anzeigen: Wenn nur der ESA-Wert vorhanden ist (z.B. nach Auslesen einer Patrouilliergruppe), wird beim "durchblättern" einer Gruppe der vorher angezeigte Graph gelöscht.

SDV 3 - 3.0.0.7 (30.05.2011)
- LogN3 Daten auslegen im Patrouilliermodus: Typischer Fehler, der während des patrouillierens auftrit, wird abgefangen. Das Patrouillieren läuft weiter.
- Menü-Import Commander 3: Importieren von Audio-Dateien möglich (Version 3), damit ist erst mal der Gruppenimport komplett, bei Audioimport wird das Erstellungsdatum als Aufnahmezeit genommen
- Veränderung LogN3 Messdaten abspeichern: Jetzt wird die Loggerzeit und nicht die aktuelle PC-Zeit genommen
- Rohrnetzplan: Iconliste im Ansichtsfenster, Arretieren gegen versehntliches verschieben der Geräte in der Karte möglich, LogN3-Messdaten anzeigen direkt aus der Karte heraus möglich, Historische Datenanzeige
- Die zusätzliche Datei "sensor_logd.ssf", die die Sensorliste für LogD enthält, wurde in das Installationsprogramm integriert (Demoifles)
- Verbesserung LogN3 Gruppenprogrammierung (Abbruch, Programmieren, Nachrichtenbehandlung)
- LogN3 Einzelprogrammierung: Verbesserte Informationen über das Programmierergebnis (wenn erfolgreich, aber auch, wenn Fehler aufgetreten sind. Das Programierfenster schließt automatisch mit dem Informationsfenster.
- Kategorien "Steptest" und "TDM" in Ribbonbar ausgeblendet, "Export" in den Kategorien "LogN3" und "LogP" ausgeblendet
- Firmwareupdate: Einzel- und Gruppenupdates möglich (LogN3, LogP, Repeater, GSMBox)
- LogN3 Messdaten einer Gruppe in einer Übersichtstabelle anzeigen (mehrere Tage, ESA-Wert-Verlauf inkl. Pegel-Frequenz in Farbe)
- LogN3: Dialog Neu: AutoDetection: IDs von LogN3 werden beim einschalten automatisch übernommen ("Automatic detection). "Automatic insert" ermöglichte das automatische einfügen, Kommentarfeld wird automatisch chronologisch ergänzt (z.B. LogN3-01 oder LogN3-02 etc.)

SDV 3 - 3.0.0.6 (18.05.2011)
- Baum: Verbesserung Gruppe löschen, wenn kein Gerät in ihr vorhanden ist.
- Menü-Import Commander 3: Verbesserung Import LogN3 aus einer Patrouiliergruppe - Import jetzt auch möglich, wenn nur der ESA-Wert vorhanden ist.
- Firmwareupdate für LogRI, LogD und LogN3 (einzelne und mehrere Geräte möglich)
- LogD Dialog GSM-Konfiguration: Verbesserung
- LogN3 Dialog Neu: Autovervollständigung für das Kommentarfeld abhängig von der LogN3-ID
- LogN3 Messdaten: Verbesserter Filter, der mehrfach speichern von Messdaten für den gleichen Tag vermeidet. Datensatz wird nur überschrieben, wenn die Daten aktueller sind (auswählbar).

SDV 3 - 3.0.0.5 (03.05.2011)
- Menü-Import Commander 3: Verbesserung Version 1: Import mehrer Gruppen gleichen Namens, Import in den Root-Ordner
- Menü-Import Commander 3: Verbesserung Import LogN3 aus einer Gruppe, Erweitert durch den Import historischer LogN3-Messdaten (Version 2, Stand 03.05.2011)
- Baum: Ordner, Gruppe, Untergruppe: Wegfall Debuginformationen nach Doppelklick
- LogN3 View: Anordnung der Steuerelemente und Anzeige verändert, Anzeige der Messwerte auf 100 Messwerte, Historische Messwerte richten sich nach der Loggerzeit
- Fehlerausgabe: Unbekannter Fehler jetzt mit Fehlercode
- Rohrnetzplan: Anzeige historischer Messwerte über ein Drop-Down-Menu

SDV 3 - 3.0.0.4 (29.04.2011)
- Internettemplates: China Mobile-NEU, Etisat (Abu Dabhi)-NEU
- LogN3 ViewData: Verbesserung Darstellung Daten (Datum)
- Kontextmenü: LogN3 Untergruppe: Gruppe "patrouillieren" statt "lesen", wenn die Gruppe als Patrolliergruppe definiert wurde.
- Geräte IDs werden in allen vorkommenden Dialogen sechstellig angezeigt (mit Nullen aufgefüllt).
- Mehrzeilige Kommentarfelder jetzt immer mit automatischem Zeilenumbruch.
- Anpassung Maximale Paketlänge für das Einlesen LogN3 Messdaten LFM
- GSMBox3 Programmieren Dialog: SMS-Zieltelfonnumern Verbesserung Numerierung. 1,2,3 statt 1,1,1
- LogN3 Gruppe Patroulieren: Verbesserung Zusammenspiel der Buttons, Bugfix (Absturz, Fenster nicht schließbar)
- Menü-Import Commander 3: Gruppen können aus einer Commander 3 Spezifischen Gruppe importiert werden (LogN3 und dazugehörige Messwerte, wenn vorhanden) (Version 1, Stand 26.04.2011)
- Integration GPS-Koordinaten für LogN3

